┃SECONDARY REMOTE CONTROL(OPTIONAL) 

Specification
Battery-powered: 2x3V CR2032 button batteries 
Working environment range 1℃~ 50℃ 

Radio frequency 433.92MHz
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Description
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The function of the secondary remote control is to turn ON/OFF the LED light    surrounding the panel.
This secondary remote control can not adjust the brightness and color of the lights.
This secondary remote control requires no wiring, you can use double-sided tape to secure it in place and use it as a wall switch..
Pair the secondary remote control with the heating device
For first-time users, the secondary remote control needs to be paired with the heating device. After powering on,press and hold the secondary remote control switch for more than 6 seconds within one minute to begin pairing.Once pairing is successful,short press the switch to control the LED light.

Notes:

Before pairing please do power off those panels which you don’t want to pair.
Pairing should be finished within 1 minute, or else you need to re-power on the heating device.
One heating device can be paired with a maximum of one main thermostat and two secondary remote controls, all of which can control the LED light.
Replace button battery
Gently press inward from the position shown in the figure below.
Forcefully pry open the casing upward.
Insert the button battery with the positive (+) symbol facing outward into the      battery slot.

Notes
Put the secondary remote control at most 5 meters from the heating device.
If the secondary remote control is disconnected, please bring the remote control close to the heating device(less than 3 meters) and repair.
No need to re-pair after replacing the battery.

If the secondary remote control fails, please replace the battery and try again.

Short press to control the LED light





pry open the casing from this point









